Name:Abdelrhman Mohaned Nasser

Section:4

Q1

1. Mask Programemd ROM

Programemd During Manufacturing

1. Programmable Reda-Only Memory (PROM)

Blow Out Fuses To Produce 0

1. Erasable Programmable ROM (EPROM)

Erase All Data By Ultra Violet Expousre

1. Electrically Erasable PROM (EEPROM)

Erase The Required Data Using An Electrical

Q2

Read/Only

Q3

Address Lines And Data Lines

Q4

1. F
2. F
3. T
4. F
5. T
6. T
7. F